$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$
$                                                                              $
$  LS-DYNA Aerospace Working Group QA Test Case 2.2                            $
$                                                                              $
$  Ballistic Impact: Fan Blade-Off Containment Test                            $
$                    Generic Soft Wall Containment                             $
$                                                                              $
$  Reference:        http://awg.lstc.com                                       $
$                                                                              $
$  Revision History:                                                           $
$                                                                              $
$                                                                              $
$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$


Description:     This QA Test Case contains a fan blade-off containment test.
                 The model contains two fan blades (the released blade and the
                 following blade), all the blade platforms, the fan containment
                 case, and the Kevlar fabric containment layer. The model
                 geometry is discretized with solid elements for the fan blades
                 and blade platforms. The fan containment housing is discretized
                 with Thick Shell elements. The fabric is discretized with one
                 layer of shell elements. 

Status:          Accepted and currently part of the AEROQA Test Suite

Classification:  Example

Keywords:        *MAT_DRY_FABRIC
                 ...

Units:           in (length), s (time), lbf-s^2/in (mass),
                 psi (stress), lbf-in (energy)

Model Data:      approx. 150778 Nodes,
                 77900 Solids, 4 Solid Materials,
                 5250 Shells, 1 Shell Material,
                 10625 Thick Shells, 1 Thick Shell Material,
                 6 Parts

Run time:        approx. total CPU time = 7 hours 52 minutes 32 seconds
                 (Intel Xeon CPU E7- 8837 @ 2.67GHz / MPP / 8 cpu's)

